

Block diagram describing power, ground, and signal connection on Arduino.

Most components are connected to a 5 V pin. Exceptions to this are the accelerometer (3.3 V) and the ESC, which is powered by a battery.

For the sonar sensors, the special data line and clock line pins are used.

We use two channels for the receiver, where channel 1 is connected to an interrupt pin (3).